SPECIAL PURPOSE DRAINS AND FITTINGS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying Special Purpose drains and fittings. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.
 
          B.      These products do not conform to or meet the requirements of ASME Standard No. A112.19.8-2007,
                    tilted “Suction Fittings for Use in Swimming Pools, Wading Pools, Spas, and Hot Tubs”. These 
                    products shall not be used in any installation in Swimming Pools, wading pools, spas, hot tubs as 
                    well as other aquatic facilities. Due to the potential endangerment from arduous and forceful suction,
                    entrapment or entanglement regardless of whether it is hair, head, limbs, or other body parts, these
                    products are prohibited from installation in these applications.

PART 2 - PRODUCTS

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a main outlet drain.

	A.	Special Purpose Drain:
		1.	Model: No. 6010 or 6020.
		2.	Description: Cast iron body and anchor flange with secured chrome plated grate and square
			frame.

**** OR ****
					
Include the following for a main outlet drain.

	A.	Special Purpose Drain:
		1.	Model: No. 6025.
		2.	Description: Cast iron side outlet body and anchor flange with secured chrome plated grate and frame.

**** OR ****
.
Include the following for a main outlet drain in sumps and pits with a reversible angle.

	A.	Special Purpose Reversible Angle Drain:
		1.	Model: No. 6040 or 6045.
		2.	Description: Cast iron body and collar with secured chrome plated angle grate and frame.

**** OR ****

Include the following for a reverse angle drain for a radius bottom.

	A.	Special Purpose Reversible Angle Drain:
		1.	Model: No. 6048.
		2.	Description: Cast iron body and collar with secured chrome plated angle grate and frame with 5” radius.

**** OR ****

Include the following for a large capacity bottom outlet drain.

	A.	Special Purpose Large Capacity Drain:
		1.	Model: No. 6050 or 6060 (Bottom Outlet)
		2.	Description: Stainless steel body and frame with loose set chrome plated grates.

**** OR ****

Include the following for a large capacity side outlet drain.

	A.	Special Purpose Large Capacity Drain:
		1.	Model: No. 6070 (Side Outlet)
		2.	Description: Stainless steel side outlet body and frame with loose set chrome plated grates.

**** OR ****

Include the following for an adjustable recirculating fitting, supply inlet for side walls.

	A.	Adjustable Recirculating Fitting:
		1.	Model: No. 6105 (SQ), 6115 (SQ), or 6125 (round).
		2.	Description: Cast iron body with secured chrome plated face with manual closure device.  Note:  6115 has no manual closure valve.  

**** OR ****

Include the following for an adjustable recirculating fitting, inlet supply for a finished wall.

	A.	Adjustable Recirculating Fitting:
		1.	Model: No. 6130.
		2.	Description: Cast iron body with secured chrome plated face and flow regulating device.

**** OR ****
						
Include the following for an adjustable recirculating fitting, inlet supply where a shallow body with provisions for flashing are required.

	A.	Adjustable Recirculating Fitting:
		1.	Model: No. 6175.
		2.	Description: Cast iron body with secured chrome plated face.

**** OR ****
					
Include the following for an adjustable recirculating fitting, inlet supply where a shallow body with provisions for flashing are required.

	A.	Adjustable Recirculating Fitting:
		1.	Model: No. 6180.
		2.	Description: Cast iron body with secured chrome plated face and shutter type manual closure.

**** OR ****
Include the following for a scum gutter drain.

	A.	Gutter Drain:
		1.	Model: No. 6200 series.
		2.	Description: Cast iron body with secured chrome plated rectangular face.

**** OR ****

Include the following for an inlet spray fitting for use in foot baths and decorative ponds.

	A.	Inlet Spray Fitting:
		1.	Model: No. 6340.
		2.	Description: Bronze body with secured chrome plated face with vertical slot openings.

**** OR ****

Include the following for a fixed standpipe overflow drain to ensure a constant water level in decorative ponds.

	A.	Overflow Drain:
		1.	Model: No. 6370.
		2.	Description: Cast iron body with chrome plated dome and 6" high standpipe.

**** OR ****

Include the following for a foot bath drain.

	A.	FootBath Drain:
		1.	Model: No. 6390.
		2.	Description: Cast iron body with chrome plated top and spanner wrench for plug removal.

**** OR ****

Include the following for a vacuum fitting.

	A.	Vacuum Cleaning Fitting:
		1.	Model: No. 6412.	
		2.	Description: Cast iron body with adjustable chrome plate bronze head with 2 inch NPT plug.

**** OR ****
				
Include the following for a hair and lint interceptor.

	A.	Hair/Lint Interceptor:
		1.	Model: No. 8790.
		2.	Description: Cast iron interceptor with removable, non-corrosive perforated strainer basket.

PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.