INTERCEPTORS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying interceptors. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS					

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.
 
Include the following for a grease interceptor for a floor or recessed installation.

	A.	Interceptor:
		1.	Model: No. 8000 series.
		2.	Description: Steel interceptor with gray duco coating inside and outside with flow control fitting.

**** OR ****

Include the following for a grease interceptor with semi-automatic draw off.

	A.	Interceptor:
		1.	Model: No. 8000GT series.
		2.	Description: Steel interceptor with gray duco coating inside and outside with steel cone, draw-off piping and valve, line shut off valve and flow control fitting.

**** OR ****

Include the following for a grease interceptor with semi-automatic draw off for a recessed installation.

	A.	Interceptor:
		1.	Model: No. 8000GTX series.
		2.	Description: Steel interceptor with gray duco coating inside and outside with flexible draw-off hose and cap, line shut off valve, and flow control fitting.

**** OR ****

Include the following for a low profile grease interceptor adaptable for dishwashers or low rough-in sinks.

	A.	Interceptor:
		1.	Model: No. 8100 series.
		2.	Description: Low profile steel interceptor with gray duco coating inside and outside with flow control fitting.

**** OR ****

Include the following for a grease interceptor in a flush with finished floor installation.

	A.	Interceptor:
		1.	Model: No. 8200 series.
		2.	Description: Steel interceptor and extension with gray duco coating inside and outside with flow control fitting.

**** OR ****

Include the following for a grease interceptor with a receiving cradle for a recessed installation.

	A.	Interceptor:
		1.	Model: No. 8300 series.
		2.	Description: Steel interceptor and receiving cradle with gray duco coating inside and outside with flow control fitting.

**** OR ****

Include the following for a grease interceptor with semi-automatic draw off and receiving cradle for a recessed installation.

	A.	Interceptor:
		1.	Model: No. 8300GT series.
		2.	Description: Steel interceptor and receiving cradle with gray duco coating inside and outside with steel cone, flexible draw-off hose and cap, line shut off valve, and flow control fitting.

**** OR ****

Include the following for a grease interceptor with semi-automatic draw off and receiving cradle for a recessed installation.

	A.	Interceptor:
		1.	Model: No. 8300GT(-W).
		2.	Description: Steel interceptor and fully enclosed receiving cradle with gray duco coating inside and outside with integral drip pan, steel cone, flexible draw-off hose and cap, line shut off valve, and flow control fitting.

**** OR ****

Include the following for a large capacity grease interceptor.

	A.	Interceptor:
		1.	Model: No. 8400 series.
		2.	Description: Steel interceptor with gray duco coating inside and outside and flow control fitting.

**** OR ****

Include the following for a large capacity grease interceptor with integral extension.

	A.	Interceptor:
		1.	Model: No. 8400E series.
		2.	Description: Steel interceptor with integral extension with gray duco coating inside and outside and flow control fitting.

**** OR ****

Include the following for an oil interceptor.

	A.	Interceptor:
		1.	Model: No. 8500 series.
		2.	Description: Steel interceptor with gray duco coating inside and outside and flow control fitting.

**** OR ****

Include the following for an oil interceptor with an integral storage compartment.

	A.	Interceptor:
		1.	Model: No. 8599.
		2.	Description: Steel interceptor with diamond plate cover, duco coating inside and coal tar outside, with flow control fitting.

**** OR ****

Include the following for a high efficiency oil/water separator.

	A.	Interceptor:
		1.	Model: No. 8600 series.
		2.	Description: Ultracept high efficiency oil/water separator.

**** OR ****

Include the following for a small capacity soilds interceptor, flush with floor or on the floor type.

	A.	Interceptor:
		1.	Model: No. 8710 series.
		2.	Description: White duco coated cast iron body and aluminum gasketed cover and sediment strainer with removable stainless steel streens.

**** OR ****

Include the following for a normal capacity soilds interceptor, flush with floor or on the floor type.

	A.	Interceptor:
		1.	Model: No. 8714 series.
		2.	Description: Steel body with galvanized sub-coat with white duco finish inside and outside, stainless steel perforated bucket and aluminum cover.

**** OR ****

Include the following for a large capacity soilds interceptor, flush with floor or on the floor type.

	A.	Interceptor:
		1.	Model: No. 8715 series.
		2.	Description: White duco coated cast iron body and aluminum gasketed cover and sediment strainer with removable stainless steel streens.

**** OR ****

Include the following for a normal capacity soilds interceptor, suspended type.

	A.	Interceptor:
		1.	Model: No. 8730 series.
		2.	Description: Suspended type white duco coated cast iron body and aluminum strainer with removable stainless steel streens.

**** OR ****

Include the following for a hair and lint interceptor.

	A.	Interceptor:
		1.	Model: No. 8750 or 8760.
		2.	Description: Chrome plated bronze body, gasketed cover and slip-type inlet elbow with perforated stainless steel basket.

**** OR ****
									
Include the following for a pipeline basket strainer for low pressure applications.

	A.	Interceptor:
		1.	Model: No. 8790.
		2.	Description: Duco coated body and cover with yoke type clamp.

**** OR ****
									
Include the following for a sand trap.

	A.	Interceptor:
		1.	Model: No. 8811.
		2.	Description: Fabricated steel catch basin, gray duco coated inside and outside, threaded inlet and outlet (with outlet trap seal).

**** OR ****
							
Include the following for a sand and sediment interceptor.

	A.	Interceptor:
		1.	Model: No. 8817.
		2.	Description: Acid resistant coated fabricated steel body and non-skid cover.

**** OR ****
		
Include the following for a lint interceptor.

	A.	Interceptor:
		1.	Model: No. 8910.
		2.	Description: Fabricated steel with gray duco coating and stainless steel primary and secondary lint screens, 3/16" diamond plate cover (secured & gasketed) and threaded inlet and outlet.

**** OR ****			
		
Include the following for a lint interceptor.

	A.	Interceptor:
		1.	Model: No. 8925.
		2.	Description: Fabricated steel body with duco coating and sediment pan w/stainless steel bucket with perforated back, secondary screen and cast iron grating.

**** OR ****	

Include the following for an open top solids interceptor to collect food waste from a indirect waste discharge line before entering the drain line going to a grease interceptor.

	A.	Interceptor:
		1.	Model: No. 8960.
		2.	Description: Fabricated type 304 stainless steel body with adjustable legs, perforated bottom bucket, and secondary poly mesh strainer.

**** OR ****
	
Include the following for a Remediator grease treatment system.

	A.	Interceptor:
		1.	Model: No. 8970.
		2.	Description: Stainless steel pretreatment unit with media and biological treatment pump with preset timer. Stainless steel solids interceptor with aluminum diamond plate cover, cast iron bridge trap and cast iron flow-control fitting.

**** OR ****

Include the following for a recessed Remediator grease treatment system.

	A.	Interceptor:
		1.	Model: No. 8970.
		2.	Description: Recessed stainless steel pretreatment unit with media and biological treatment pump with preset timer. Recessed stainless steel solids interceptor with aluminum diamond plate cover, cast iron bridge trap and cast iron flow-control fitting.

**** OR ****

Include the following for a Grease+Gard inline solids interceptor to collect food solids before entering the drain line going to a grease interceptor.

	A.	Interceptor:
		1.	Model: No. 8980.
		2.	Description: Stainless steel body with adjustable legs, perforated bottom bucket, secondary poly mesh strainer and secured cover.

PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.