SANITARY FLOOR, AREA AND INDIRECT WASTE DRAINS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying sanitary floor, area and indirect waste drains. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL											 

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS					

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting Jay R. Smith Mfg. Co. specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a stainless steel indirect waste receptor in a foot/light traffic area where sanitation, corrosion resistance, durability and longevity are required.

	A.	Drain:
		1.	Model: No. 3001-3004.
		2.	Description: Stainless steel 12 inch square top with stainless steel loose set grate and perforated dome bottom strainer.
					
**** OR ****

Include the following for a stainless steel indirect waste receptor in a foot/light traffic area where sanitation, corrosion resistance, durability and longevity are required.

	A.	Drain:
		1.	Model: No. 3006-3009.
		2.	Description: Stainless steel 12 inch square top with stainless steel loose set grate and sediment bucket.
					
**** OR ****

Include the following for a wide flange sani-ceptor for use where the floor or deck will be surfaced with troweled composition elastomeric covering.

	A.	Drain:
		1.	Model: No. DX3001-DX3004.
		2.	Description: Stainless steel 12 inch square raised rim top with wide flange body, stainless steel ribbed non-tilt loose set grate and perforated dome bottom strainer.

**** OR ****

Include the following for a wide flange sani-ceptor for use where the floor or deck will be surfaced with troweled composition elastomeric covering.

	A.	Drain:
		1.	Model: No. DX3006-DX3009.
		2.	Description: Stainless steel 12 inch square raised rim top with wide flange body, stainless steel ribbed non-tilt loose set grate and sediment bucket.

**** OR ****	
							
Include the following for an indirect waste receptor with a nickel bronze top for use in a traffic area where sanitation, corrosion resistance, durability and longevity are required.

	A.	Drain:
		1.	Model: No. 3001NB-3004NB.
		2.	Description: Stainless steel 12 inch square-top with nickel bronze frame and secured grate, and stainless steel perforated dome bottom strainer.

**** OR ****	
							
Include the following for an indirect waste receptor with a nickel bronze top for use in a traffic area where sanitation, corrosion resistance, durability and longevity are required.

	A.	Drain:
		1.	Model: No. 3006NB-3009NB.
		2.	Description: Stainless steel 12 inch square-top with nickel bronze frame and secured grate, and stainless steel sediment bucket.

**** OR ****
							
Include the following for a shallow type sanitary floor receptor where small capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3020.
		2.	Description: Cast iron 8-1/2 inch diameter flanged receptor with seepage holes and acid resistant coated interior with nickel bronze secured grate and rim, and aluminum dome bottom strainer.

**** OR ****
												
Include the following for a shallow type sanitary floor receptor where small capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3021.
		2.	Description: Cast iron 8-1/2 inch diameter flanged receptor with seepage holes and acid resistant coated interior with nickel bronze secured grate and rim, and aluminum sediment bucket.

**** OR ****		
Include the following for a shallow type sanitary floor receptor where medium capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3030.
		2.	Description: Cast iron 12-1/2 inch diameter flanged receptor with seepage holes and acid resistant coated interior with nickel bronze secured grate and rim, and aluminum dome bottom strainer.

 	**** OR ****		

Include the following for a shallow type sanitary floor receptor where medium capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3031.
		2.	Description: Cast iron 12-1/2 inch diameter flanged receptor with seepage holes and acid resistant coated interior with nickel bronze secured grate and rim, and aluminum sediment bucket.
														
**** OR ****
							
Include the following for a sanitary floor receptor where medium capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3040.
		2.	Description: Cast iron 8-1/2 inch diameter flanged receptor with seepage holes and acid resistant coated interior with nickel bronze secured grate and rim, and aluminum dome bottom strainer.

**** OR ****
							
Include the following for a sanitary floor receptor where medium capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3041.
		2.	Description: Cast iron 8-1/2 inch diameter flanged receptor with seepage holes and acid resistant coated interior with nickel bronze secured grate and rim, and aluminum sediment bucket.

**** OR ****

Include the following for an open top, single overhead discharge indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3040 (-10).
		2.	Description: Cast iron 8 inch diameter open top receptor with acid resistant coated interior and aluminum dome bottom strainer.		

**** OR ****

Include the following for a deep sanitary floor receptor where normal traffic and high capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3060.
		2.	Description: Cast iron 12-1/2 inch diameter receptor with seepage holes and acid resistant coated interior with nickel bronze rim, secured top grate, and aluminum dome bottom strainer. 
				
**** OR ****

Include the following for a deep sanitary floor receptor where normal traffic and high capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3061.
		2.	Description: Cast iron 12-1/2 inch diameter receptor with seepage holes and acid resistant coated interior with nickel bronze rim, secured top grate, and aluminum sediment bucket. 
							
**** OR ****
							
Include the following for a wide flange sanitary floor drain where waterproof traffic floor coverings are applied.

	A.	Drain:
		1.	Model: No. DX3027.
		2.	Description: Cast iron 8 1/2 inch diameter wide flange receptor with acid resistant coated interior and nickel bronze top with sediment bucket.  

**** OR ****
							
Include the following for a wide flange sanitary floor drain where waterproof traffic floor coverings are applied.

	A.	Drain:
		1.	Model: No. DX3068.
		2.	Description: Cast iron 12 1/2 inch diameter wide flange receptor with acid resistant coated interior and nickel bronze top with sediment bucket.  

**** OR ****

Include the following for a square top sanitary floor drain where normal capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3100.
		2.	Description: Cast iron 8-1/2 inch square drain with acid resistant coated interior with nickel bronze secured grate and rim, and aluminum dome bottom strainer. 

**** OR ****

Include the following for a square top sanitary floor drain where normal capacity drainage is anticipated.

	A.	Drain:
		1.	Model: No. 3101.
		2.	Description: Cast iron 8-1/2 inch square drain with acid resistant coated interior with nickel bronze secured grate and rim, and aluminum sediment bucket. 

**** OR ****

Include the following for a open top, single overhead discharge, indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3100(-10).
		2.	Description: Cast iron 8 inch square open top receptor with acid resistant coated interior and aluminum dome bottom strainer.
					
**** OR ****

Include the following for an indirect waste receptor under low cabinets.

	A.	Drain:
		1.	Model: No. 3100(-15).
		2.	Description: Cast iron 8-1/2 inch square receptor with acid resistant coated interior and nickel bronze recessed top grate and aluminum dome bottom strainer.

**** OR ****

Include the following for an indirect waste receptor in quarry tile.

	A.	Drain:
		1.	Model: No. 3110 (6 inch deep), 3120 (8 inch deep) or 3130 (10 inch deep).
		2.	Description: Cast iron 6 inch deep x 12 inch square receptor with acid resistant coated interior, extra thick nickel bronze rim and top grate, and aluminum dome bottom strainer.
			
**** OR ****

Include the following for an indirect waste receptor in quarry tile.

	A.	Drain:
		1.	Model: No. 3110 (6 inch deep), 3120 (8 inch deep) or 3130 (10 inch deep).
		2.	Description: Cast iron 12 inch square receptor with acid resistant coated interior, extra thick nickel bronze rim and secured top grate, and aluminum dome bottom strainer.

					**** OR ****

Include the following for an indirect waste receptor in quarry tile.

	A.	Drain:
		1.	Model: No. 3111 (6 inch deep), 3121 (8 inch deep) or 3131 (10 inch deep).
		2.	Description: Cast iron 12 inch square receptor with acid resistant coated interior, extra thick nickel bronze rim and secured top grate, and aluminum sediment bucket.
														
**** OR ****

Include the following for an indirect waste receptor where normal traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3140 (6 inch deep), 3150 (8 inch deep), or 3160 (10 inch deep).
		2.	Description: Cast iron 12-1/2 inch square receptor with acid resistant coated interior, nickel bronze rim and top grate, and aluminum dome bottom strainer.
												
**** OR ****

Include the following for a open top, multiple overhead discharge, indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3150(-10).
		2.	Description: Cast iron 12-1/2 inch square, 8 inch deep open top receptor with acid resistant coated interior, and aluminum dome bottom strainer. 
						
**** OR ****

Include the following for an indirect waste receptor in a kitchen or counter curb.

	A.	Drain:
		1.	Model: No. 3150(-18).
		2.	Description: Cast iron 12-1/2 inch square, 8 inch deep receptor with acid resistant coated interior and nickel bronze rim and angle top grate with aluminum dome bottom strainer. 

**** OR ****

Include the following for an indirect waste receptor where normal traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3141 (6 inch deep), 3151 (8 inch deep), or 3161 (10 inch deep).
		2.	Description: Cast iron 12-1/2 inch square receptor with acid resistant coated interior, nickel bronze rim and top grate, and aluminum sediment bucket.

**** OR ****

Include the following for an indirect waste receptor in a kitchen floor.

	A.	Drain:
		1.	Model: No. 3161 (-19).
		2.	Description: Cast iron 12-1/2 inch square, 10 inch deep receptor with acid resistant coated interior and nickel bronze rim and hinged top grate with stainless steel 1/4 inch mesh lined aluminum sediment bucket.

**** OR ****

Include the following for a large capacity indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3200.
		2.	Description: Cast iron 16-1/2 inch square, 12 inch deep receptor with acid resistant coated interior and nickel bronze rim, hinged top grate, and aluminum dome bottom strainer.
								
**** OR ****

Include the following for a large capacity indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3201.
		2.	Description: Cast iron 16-1/2 inch square, 12 inch deep receptor with acid resistant coated interior and nickel bronze rim, hinged top grate, and aluminum sediment bucket.

**** OR ****

Include the following for an extra large capacity indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3250.
		2.	Description: Fabricated steel 24 inch by 12 inch flanged receptor with acid resistant coated interior and nickel bronze rim, secured grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for an extra large capacity indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3251.
		2.	Description: Fabricated steel 24 inch by 12 inch flanged receptor with acid resistant coated interior and nickel bronze rim, secured grate, and aluminum sediment bucket.

**** OR ****

Include the following for a small capacity indirect waste drain.

	A.	Drain:
		1.	Model: No. 3300.
		2.	Description: Cast iron 4 inch by 8 inch flanged receptor with acid resistant coated interior, nickel bronze rim, secured grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a small capacity indirect waste drain.

	A.	Drain:
		1.	Model: No. 3301.
		2.	Description: Cast iron 4 inch by 8 inch flanged receptor with acid resistant coated interior, nickel bronze rim, secured grate, and aluminum sediment bucket.

**** OR ****

Include the following for a medium capacity indirect waste drain.

	A.	Drain:
		1.	Model: No. 3320.
		2.	Description: Cast iron 6 inch by 12 inch flanged receptor with acid resistant coated interior, nickel bronze rim, secured grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a medium capacity indirect waste drain.

	A.	Drain:
		1.	Model: No. 3321.
		2.	Description: Cast iron 6 inch by 12 inch flanged receptor with acid resistant coated interior, nickel bronze rim, secured grate, and aluminum sediment bucket.

**** OR ****

Include the following for a drain for waste from refrigerators or similar appliances.

	A.	Drain:
		1.	Model: No. 3365
		2.	Description: Cast iron body with acid resistant coated interior and recessed nickel bronze top. 

**** OR ****

Include the following for a cast iron sanitary can washing floor drain.

	A.	Drain:
		1.	Model: No. 3370.
		2.	Description: Cast iron body with acid resistant coated interior, nickel bronze rim and grate, free standing aluminum bucket with ported openings lined with 1/4 inch staiinless steel mesh and chrome plated bronze adjustable nozzle assembly.
								
**** OR ****

Include the following for a stainless steel sanitary can washing floor drain.

	A.	Drain:
		1.	Model: No. 3371.
		2.	Description: Stainless steel body, stainless steel grate, free standing aluminum bucket with ported openings lined with 1/4 inch stainless steel mesh and chrome plated bronze adjustable nozzle assembly.

**** OR ****

Include the following for a water supply control box to supply hot, cold or tempered water to can washing drains, flushing rim drains or other devices requiring a water supply, to be mounted flush with a plaster wall.

	A.	Control Box:
		1.	Model: No. 3380.
		2.	Description: Flush mounted stainless steel box with cylinder type key lock and piano hinged cover, bronze control valves, bronze screwdriver stops and bronze atmospheric type vacuum breaker.

**** OR ****

Include the following for a water supply control box to supply hot, cold or tempered water to can washing drains, flushing rim drains or other devices requiring a water supply, to be surface mounted.

	A.	Control Box:
		1.	Model: No. 3385.
		2.	Description: Surface mounted stainless steel box with cylinder type key lock and piano hinged cover, bronze control valves, bronze screwdriver stops and bronze atmospheric type vacuum breaker.

**** OR ****

Include the following for a large capacity indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3400.
		2.	Description: Cast iron 12 inch diameter, 8 inch deep receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a large capacity indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3401.
		2.	Description: Cast iron 12 inch diameter, 8 inch deep receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for an open top, multiple overhead discharge indirect waste receptor.

	A.	Drain:
		1.	Model: No. 3400 (-10).
		2.	Description: Cast iron 12 inch diameter, 8 inch deep open top receptor with acid resistant coated interior and aluminum dome bottom strainer.

**** OR ****

Include the following for a shallow, large capacity, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3402.
		2.	Description: Cast iron 12 inch diameter, 3 inch deep receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a shallow, large capacity, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3412.
		2.	Description: Cast iron 12 inch diameter, 3 inch deep receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for a medium capacity, square top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3410.
		2.	Description: Cast iron 8 inch square, 6 inch deep flanged receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a medium capacity, square top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3411.
		2.	Description: Cast iron 8 inch square, 6 inch deep flanged receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for a large capacity, square top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3420 (6 inch deep), 3430 (8 inch deep), or 3440 (10 inch deep).
		2.	Description: Cast iron 12 inch square flanged receptor with seepage holes, acid resistant coated interior and loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a large capacity, square top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3421 (6 inch deep), 3431 (8 inch deep), or 3441 (10 inch deep).
		2.	Description: Cast iron 12 inch square flanged receptor with seepage holes, acid resistant coated interior and loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****
														
Include the following for a large capacity, square top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:				
		1.	Model: No. 3450.
		2.	Description: Cast iron 16 inch square, 12 inch deep flanged receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****
														
Include the following for a large capacity, square top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:				
		1.	Model: No. 3451.
		2.	Description: Cast iron 16 inch square, 12 inch deep flanged receptor with seepage holes, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for a shallow, rectangular top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3460.
		2.	Description: Cast iron 4 inch by 8 inch, 3 1/4 inch deep flanged receptor, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.
										
**** OR ****

Include the following for a shallow, rectangular top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3461.
		2.	Description: Cast iron 4 inch by 8 inch, 3 1/4 inch deep flanged receptor, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for a shallow, rectangular top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3470.
		2.	Description: Cast iron 6 inch by 12 inch, 7 1/2 inch deep flanged receptor, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for a shallow, rectangular top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:
		1.	Model: No. 3471.
		2.	Description: Cast iron 6 inch by 12 inch, 7 1/2 inch deep flanged receptor, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for an extra deep, rectangular top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:				
		1.	Model: No. 3482.
		2.	Description: Fabricated steel 24 inch by 12 inch, 17 inch deep flanged receptor, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum dome bottom strainer.

**** OR ****

Include the following for an extra deep, rectangular top, indirect waste receptor where no traffic is anticipated.

	A.	Drain:				
		1.	Model: No. 3483.
		2.	Description: Fabricated steel 24 inch by 12 inch, 17 inch deep flanged receptor, acid resistant coated interior, loose set acid resistant coated cast iron grate, and aluminum sediment bucket.

**** OR ****

Include the following for a funnel-ceptor drain with an adjustable strainer head to receive waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3510 Series.
		2.	Description: Cast iron body and flashing collar with adjustable strainer head, secured square hole grate, and funnel.

**** OR ****

Include the following for a bottom outlet funnel-ceptor drain with an adjustable round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3610.
		2.	Description: Bottom outlet cast iron flanged receptor and flashing collar with adjustable top, medium duty bar grate, and round funnel.

**** OR ****

Include the following for a side outlet funnel-ceptor drain with an adjustable round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3620.
		2.	Description: Side outlet cast iron flanged receptor and flashing collar with adjustable top, medium duty bar grate, and round funnel.		

**** OR ****

Include the following for a bottom outlet funnel-ceptor drain with an adjustable round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3650 (8 1/2 inch diameter top) or 3655 (12 1/2 inch diameter top).
		2.	Description: Bottom outlet cast iron flanged receptor and flashing collar with adjustable top, medium duty bar grate, and oval funnel.
				
**** OR ****

Include the following for a side outlet funnel-ceptor drain with an adjustable round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3660 (8 1/2 inch diameter top) or 3665 (12 1/2 inch diameter top).
		2.	Description: Side outlet cast iron flanged receptor and flashing collar with adjustable top, medium duty bar grate, and oval funnel.
												
**** OR ****

Include the following for a bottom outlet funnel-ceptor drain with a round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3710.
		2.	Description: Bottom outlet cast iron flanged receptor and flashing collar, medium duty bar grate, and round funnel.

**** OR ****

Include the following for a side outlet funnel-ceptor drain with a round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3720.
		2.	Description: Side outlet cast iron flanged receptor and flashing collar, medium duty bar grate, and round funnel.

**** OR ****

Include the following for a bottom outlet funnel-ceptor drain with a round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3750 (8 1/2 inch diameter top) or 3755 (12 1/2 inch diameter top).
		2.	Description: Bottom outlet cast iron flanged receptor and flashing collar, medium duty bar grate, and oval funnel.		
			
**** OR ****

Include the following for a side outlet funnel-ceptor drain with a round top to receive drip, condensate, or waste water from indirect waste lines.

	A.	Drain:				
		1.	Model: No. 3760 (8 1/2 inch diameter top) or 3765 (12 1/2 inch diameter top).
		2.	Description: Side outlet cast iron flanged receptor and flashing collar, medium duty bar grate, and oval funnel.			

**** OR ****

Include the following for an acid resistant coated cast iron drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water.

	A.	Funnel:				
		1.	Model: No. 3811.
		2.	Description: Cast iron funnel with acid resistant coated interior and exterior.		
			
**** OR ****

Include the following for an acid resistant coated cast iron drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water, and a ‘p’ trap is needed to prevent sewer gases from entering the room.

	A.	Funnel:				
		1.	Model: No. 3821.
		2.	Description: Cast iron funnel and ‘p’ trap with acid resistant coated interior or exterior.

**** OR ****		

Include the following for a duco coated cast iron drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water.

	A.	Funnel:				
		1.	Model: No. 3812.
		2.	Description: Duco coated cast iron funnel.		
		
**** OR ****		

Include the following for a duco coated cast iron drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water, and a ‘p’ trap is needed to prevent sewer gases from entering the room.					

	A.	Funnel:				
		1.	Model: No. 3822.
		2.	Description: Duco coated cast iron funnel and ‘p’ trap.		
	
**** OR ****		

Include the following for a bronze drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water.

	A.	Funnel:				
		1.	Model: No. 3813.
		2.	Description: Cast bronze funnel.	

**** OR ****		

Include the following for a bronze drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water, and a ‘p’ trap is needed to prevent sewer gases from entering the room.					

	A.	Funnel:				
		1.	Model: No. 3823.
		2.	Description: Cast bronze funnel and ‘p’ trap.	

**** OR ****		

Include the following for a chrome plated drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water.

	A.	Funnel:				
		1.	Model: No. 3814.
		2.	Description: Polished chrome plated cast bronze funnel.	

**** OR ****		

Include the following for a chrome plated drip and condensate funnel where indirect waste lines above the floor require receptors to receive drip, condensate, or waste water, and a ‘p’ trap is needed to prevent sewer gases from entering the room.					

	A.	Funnel:				
		1.	Model: No. 3824.
		2.	Description: Polished chrome plated cast bronze funnel and ‘p’ trap.

**** OR ****
Include the following for a fixed air gap.				

	A.	Fixed Air Gap:
		1.	Model: No. 3950 or 3955.
		2.	Description: Cast iron fixed air gap.
**** OR ****

Include the following for a roof drain to receive waste water from air conditioning units, cooling towers and other mechanical equipment.				

	A.	Drain:
		1.	Model: No. 3960, 3970, or 3980.
		2.	Description: Cast iron receptor with solid water dam and cast iron dome bottom strainer secured with stainless steel vandal proof screws.

PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.