LAVATORY AND SINK SUPPORTS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying lavatory supports. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS													

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a floor support with concealed arms for a high-back lavatory in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0700 series.
		2.	Description: Fixture support with concealed adjustable arms and “Sure-Set” mechanical locking device, and round steel uprights with welded bases.

**** OR ****

Include the following for a floor support with concealed arms for a flat-slab lavatory in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0700 (-E) series.
		2.	Description: Fixture support with chromium plated threaded escutcheons, concealed adjustable arms and “Sure-Set” mechanical locking device, and round steel uprights with welded bases. 

**** OR ****

Include the following for a floor support with concealed arms for a high-back lavatory with labor saver uprights.

	A.	Lavatory Support:
		1.	Model: No. 0710 series.
		2.	Description: Fixture support with concealed adjustable arms and “Sure-Set” mechanical locking device, and round steel, labor saver, uprights with welded bases.

**** OR ****

Include the following for a floor support with concealed arms for a flat-slab lavatory with labor saver uprights.

	A.	Lavatory Support:
		1.	Model: No. 0710 (-E) series.
		2.	Description: Fixture support with chromium plated threaded escutcheons, concealed adjustable arms and “Sure-Set” mechanical locking device, and round steel, labor saver, uprights with welded bases. 

**** OR ****

Include the following for a wall mounted support with concealed arms for a high-back lavatory.

	A.	Lavatory Support:
		1.	Model: No. 0720 series.
		2.	Description: Fixture support with concealed adjustable arms and “Sure-Set” mechanical locking device.

**** OR ****

Include the following for a wall mounted support with concealed arms for a flat-slab lavatory.

	A.	Lavatory Support:
		1.	Model: No. 0720 (-E) series.
		2.	Description: Fixture support with chromium plated threaded escutcheons, concealed adjustable arms and “Sure-Set” mechanical locking device. 

**** OR ****

Include the following for a floor mounted support with exposed arms for a high-back or flat-slab lavatory in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0750.
		2.	Description: Fixture support with exposed, acid resistant coated, arms and round steel uprights with welded bases.

**** OR ****
				
Include the following for a floor mounted support with exposed arms for a high-back enameled iron lavatory in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0752.
		2.	Description: Fixture support with exposed, offset, arms and round steel uprights with welded bases.

**** OR ****

Include the following for a floor mounted support with exposed arms and labor saver uprights for a high-back or flat-slab lavatory.

	A.	Lavatory Support:
		1.	Model: No. 0760.
		2.	Description: Fixture support with exposed, acid resistant coated, arms and round steel, labor saver, uprights with welded bases.

**** OR ****
				
Include the following for a floor mounted support with exposed arms and labor saver uprights for a high-back enameled iron lavatory.

	A.	Lavatory Support:
		1.	Model: No. 0762.
		2.	Description: Fixture support with exposed, offset, arms and round steel, labor saver, uprights with welded bases.

**** OR ****

Include the following for a wall mounted support with exposed arms for a high-back or flat-slab lavatory set on a masonry or stud wall.

	A.	Lavatory Support:
		1.	Model: No. 0770.
		2.	Description: Fixture support with exposed, acid resistant coated, arms.

**** OR ****
				
Include the following for a wall mounted support with exposed arms for a high-back enameled iron lavatory set on a masonry or stud wall.

	A.	Lavatory Support:
		1.	Model: No. 0772.
		2.	Description: Fixture support with exposed, offset, acid resistant coated, arms.	

**** OR ****

Include the following for a wall mounted support with exposed arms for a high-back or flat-slab lavatory set on a block wall.

	A.	Lavatory Support:
		1.	Model: No. 0780.
		2.	Description: Fixture support with exposed, acid resistant coated, arms.

**** OR ****
								
Include the following for a wall mounted support with exposed arms for a high-back enameled iron lavatory set on a block wall.

	A.	Lavatory Support:
		1.	Model: No. 0782.
		2.	Description: Fixture support with exposed, offset, acid resistant coated, arms.	
				
**** OR ****

Include the following for a wall mounted support with exposed arms for a high-back or flat-slab lavatory to attach to a backing plate secured in the wall.

	A.	Lavatory Support:
		1.	Model: No. 0790.
		2.	Description: Fixture support with exposed, acid resistant coated, arms.

**** OR ****
								
Include the following for a wall mounted support with exposed arms for a high-back enameled iron lavatory to attach to a backing plate secured in the wall.

	A.	Lavatory Support:
		1.	Model: No. 0792.
		2.	Description: Fixture support with exposed, offset, acid resistant coated, arms.	
					
**** OR ****
								
Include the following for a floor mounted support with a concealed hanger for a high-back lavatory in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0800.
		2.	Description: Fixture support with concealed hanger and round steel uprights with welded bases.
			
**** OR ****
												
Include the following for a floor mounted support with a concealed hanger and labor saver uprights for a high-back lavatory.

	A.	Lavatory Support:
		1.	Model: No. 0801.
		2.	Description: Fixture support with concealed hanger and round steel, labor saver, uprights with welded bases.	
			
**** OR ****
		
Include the following for a floor mounted support with a concealed hanger and extended bottom securing lugs for a high-back lavatory in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0805.
		2.	Description: Fixture support with concealed hanger, extended bottom securing lugs, and round steel uprights with welded bases.	

**** OR ****
		
Include the following for a floor mounted support with a concealed wall bracket for multiple drinking fountains in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0823.
		2.	Description: Fixture support with concealed wall bracket, and round steel uprights with welded bases.	

**** OR ****
		
Include the following for a floor mounted support with a concealed hanger for a small drinking fountain in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0824.
		2.	Description: Fixture support with integral concealed hanger, and round steel uprights with welded bases.		

**** OR ****
		
Include the following for a wall mounted support with a concealed hanger for high back lavatories.

	A.	Lavatory Support:
		1.	Model: No. 0825 or No. 0826.
		2.	Description: Reinforcing plate with integral concealed hanger.

**** OR ****
		
Include the following for a wall mounted support with a concealed hanger for a wash down urinal.

	A.	Lavatory Support:
		1.	Model: No. 0827 or No. 0828.
		2.	Description: Reinforcing plate with integral concealed hanger.
	
**** OR ****
		
Include the following for a floor mounted support with concealed hangers for off the floor electric water coolers in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0830.
		2.	Description: Fixture support with integral concealed hangers, and round steel uprights with welded bases.		
**** OR ****
		
Include the following for a floor mounted support with concealed hangers and labor saver uprights for off the floor electric water coolers.

	A.	Lavatory Support:
		1.	Model: No. 0831.
		2.	Description: Fixture support with integral concealed hangers, and round steel, labor saver, uprights with welded bases.		

**** OR ****
		
Include the following for a floor mounted support with concealed hangers for high back institutional type lavatories in metal stud construction.

	A.	Lavatory Support:
		1.	Model: No. 0844.
		2.	Description: Fixture support with integral concealed hangers, and round steel uprights with welded bases.	
	
**** OR ****
		
Include the following for a floor mounted support with exposed arms for heavy washup sinks.

	A.	Lavatory Support:
		1.	Model: No. 0850 or No. 0851.
		2.	Description: Fixture support with acid resistant coated exposed arms, a fixture mounting plate, and round steel uprights with welded bases.	

**** OR ****
		
Include the following for a heavy duty floor mounted support with exposed arms for kitchen and service sinks.

	A.	Lavatory Support:
		1.	Model: No. 0870.
		2.	Description: Heavy duty fixture support with acid resistant coated exposed arms and round steel uprights with welded bases.	

**** OR ****
		
Include the following for a heavy duty floor mounted support with exposed arms for enamel iron service sinks with cast iron lugs under basin.

	A.	Lavatory Support:
		1.	Model: No. 0871.
		2.	Description: Heavy duty fixture support with offset, acid resistant coated, exposed arms and round steel uprights with welded bases.	
		
**** OR ****
		
Include the following for a heavy duty floor mounted support for surgical scrub up and flushing rim sink.

	A.	Lavatory Support:
		1.	Model: No. 0913 or No. 0914.
		2.	Description: Heavy duty fixture support with supporting studs and adjustable coupling and round steel uprights with welded bases.		

**** OR ****
		
Include the following for a heavy duty floor mounted support for back outlet surgical scrub up and flushing rim sink.

	A.	Lavatory Support:
		1.	Model: No. 0915.
		2.	Description: Heavy duty fixture support with supporting studs, adjustable coupling, and waste fitting, and round steel uprights with welded bases.	

**** OR ****
		
Include the following for a heavy duty floor mounted support with labor saver uprights for surgical scrub up and flushing rim sink.

	A.	Lavatory Support:
		1.	Model: No. 0923 or No. 0924.
		2.	Description: Heavy duty fixture support with supporting studs and adjustable coupling and round steel, labor saver, uprights with welded bases.		

**** OR ****
		
Include the following for a heavy duty floor mounted support for back outlet surgical scrub up and flushing rim sink.

	A.	Lavatory Support:
		1.	Model: No. 0925.
		2.	Description: Heavy duty fixture support with supporting studs, adjustable coupling, and waste fitting, and round steel, labor saver, uprights with welded bases.	
														
PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.