Thermostatic Hi-Lo Mixing Valve Supply Fixture

SFMV-1-B-OT-CWB-ITG
1/2" Inlets, 1/2" Outlet 15 GPM (56.8 LPM); Bottom Inlet; Top Outlet, Cold Water Bypass, Inlet Temperature Gauge

SMV2-T-OT-SMC-PRC
3/4" Inlets, 1" Outlet 45 GPM (170 LPM); Top Inlets; Top Outlet, Surface Mount Cabinet with Prime Coat Finish (16 gauge mild steel)

SFMV-2-B-OT-ITG
3/4" Inlets, 1" Outlet 45 GPM (170 LPM); Bottom Inlets; Top Outlet, Inlet Temperature Gauge

SFMV-2-B-OT-ITG-RC-PRC-DRS-L
3/4" Inlets, 1" Outlet 45 GPM (170 LPM); Bottom Inlets; Top Outlet, Inlet Temperature Gauge, Recessed Cabinet with Prime Coat Finish (16 gauge mild steel), Solid Door for Valve Supply Fixture Cabinet, Door Hinge on Left Side

SFMV-2-B-OT-ITG-SMC-PRC-DRS-L
3/4" Inlets, 1" Outlet 45 GPM (170 LPM); Bottom Inlets; Top Outlet, Inlet Temperature Gauge, Surface Mount Cabinet with Prime Coat Finish (16 gauge mild steel), Solid Door for Valve Supply Fixture Cabinet, Door Hinge on Left Side

SFMV-3-B-OT
Brass Valve Bodyl1” Inlets & 1-1/4” Outlet 90 GPM (341 LPM); Bottom Inlet; Top Outlet

SFMV-3-B-OT-ITG
1” Inlets & 1-1/4” Outlet 90 GPM (341 LPM); Bottom Inlet; Top Outlet; Inlet Temperature Gauge, Hot & Cold

SFMV-4-B-OT-ITG-RC-PRC
Brass Valve Body , 1-1/4” Inlets & 1-1/2” Outlet 150 GPM (568 LPM); Bottom Inlet; Top Outlet; Inlet Temperature Gauge, Hot & Cold; Recessed Cabinet with Prime Coat Finish (16 gauge mild steel)

SFMV_Series_Valve_Supply_Fixture_DWG.txt
List of contents in this zip file

