CLEANOUTS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying cleanouts. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a cleanout in a finished room floor.

	A.	Cleanout:
		1.	Model: No. 4020 series.
		2.	Description: Cast iron floor level cleanout assembly with round, adjustable, scoriated, nickel bronze top, and no-hub outlet.

**** OR ****

Include the following for a cleanout in a carpeted floor.

	A.	Cleanout:
		1.	Model: No. 4020 (-X) 
		2.	Description: Cast iron floor level cleanout assembly with round, adjustable, scoriated, nickel bronze top and carpet clamping frame, and no-hub outlet.

**** OR ****

Include the following for a cleanout with a speedi-set outlet in a carpeted floor.

	A.	Cleanout:
		1.	Model: No. 4031 (-X)
		2.	Description: Cast iron floor level cleanout assembly with round, adjustable, scoriated, nickel bronze top with carpet clamping frame, and a speedi-set outlet.

**** OR ****

Include the following for a round top cleanout with an inside caulk outlet in a finished room floor.

	A.	Cleanout:
		1.	Model: No. 4025 series.
		2.	Description: Cast iron floor level cleanout assembly with round, adjustable, scoriated, nickel bronze top with an inside caulk outlet.

**** OR ****

Include the following for a round top cleanout with a speedi-set outlet in a finished room floor.

	A.	Cleanout:
		1.	Model: No. 4031 series.
		2.	Description: Cast iron floor level cleanout assembly with round, adjustable, scoriated, nickel bronze top, and a speedi-set outlet.

**** OR ****

Include the following for a square top cleanout with a no-hub outlet in a finished floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4040 series.
		2.	Description: Cast iron cleanout with square, adjustable, scoriated, secured nickel bronze top, and no-hub outlet.

**** OR ****

Include the following for a square top cleanout with an inside caulk outlet in a finished floor with foot and medium load wheeled traffic

	A.	Cleanout:
		1.	Model: No. 4045 series.
		2.	Description: Cast iron cleanout with square, adjustable, scoriated, secured nickel bronze top and inside caulk outlet. 

**** OR ****

Include the following for a square top cleanout with a speedi-set outlet in a finished floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4051 or 4053 series.
		2.	Description: Cast iron cleanout with square, adjustable, scoriated, secured nickel bronze top and a speedi-set outlet.

**** OR ****

Include the following for a cleanout with a no-hub outlet in a finished floor of a hospital, school, or an institutional or industrial building with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4100 series.
		2.	Description: Cast iron cleanout with extra heavy duty round, adjustable, scoriated, secured nickel bronze top, and no-hub outlet.

**** OR ****

Include the following for a cleanout with an inside caulk outlet in a finished floor of a hospital, school, or an institutional or industrial building with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4105 series.
		2.	Description: Cast iron cleanout with extra heavy duty round, adjustable, scoriated, secured nickel bronze top and an inside caulk outlet.

**** OR ****

Include the following for a cleanout with a speedi-set outlet in a finished floor of a hospital, school, or an institutional or industrial building with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4111 series.
		2.	Description: Cast iron cleanout with extra heavy duty round, adjustable, scoriated, secured nickel bronze top and a speedi-set outlet.

**** OR ****

Include the following for a cleanout with a no-hub outlet in a finished floor subject to pedestrian traffic when a threaded, watertight cover is desired.

	A.	Cleanout:
		1.	Model: No. 4120 series.
		2.	Description: Cast iron cleanout with round, adjustable, scoriated, nickel bronze top with threaded spanner wrench cover, and no-hub outlet.

**** OR ****

Include the following for a cleanout with an inside caulk outlet in a finished floor subject to pedestrian traffic when a threaded, watertight cover is desired.

	A.	Cleanout:
		1.	Model: No. 4125 series.
		2.	Description: Cast iron cleanout with round, adjustable, scoriated nickel bronze top with threaded spanner wrench cover and an inside caulk outlet.

**** OR ****

Include the following for a cleanout with a speedi-set outlet in a finished floor subject to pedestrian traffic when a threaded, watertight cover is desired.

	A.	Cleanout:
		1.	Model: No. 4131 series.
		2.	Description: Cast iron cleanout with round, adjustable, scoriated nickel bronze top with threaded spanner wrench cover, and a speedi-set outlet.

**** OR ****

Include the following for a round top cleanout with a no-hub outlet in a linoleum or asphalt tile floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4140 series.
		2.	Description: Cast iron floor level cleanout assembly with a round adjustable nickel bronze top with 1/8 inch tile recess, and no-hub outlet.

**** OR ****

Include the following for a round top cleanout with an inside caulk outlet in a linoleum or asphalt tile floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4145 series.
		2.	Description: Cast iron floor level cleanout assembly with a round adjustable nickel bronze top with 1/8 inch tile recess and an inside caulk outlet.

**** OR ****

Include the following for a round top cleanout with a speedi-set outlet in a linoleum or asphalt tile floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4151 series.
		2.	Description: Cast iron floor level cleanout assembly with a round adjustable nickel bronze top with 1/8 inch tile recess, and a speedi-set outlet.

**** OR ****

Include the following for a square top cleanout with a no-hub outlet in a linoleum or asphalt tile floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4160 series.
		2.	Description: Cast iron floor level cleanout assembly with a square adjustable nickel bronze top with 1/8 inch tile recess, and no-hub outlet.

**** OR ****

Include the following for a square top cleanout with an inside caulk outlet in a linoleum or asphalt tile floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4165 series.
		2.	Description: Cast iron floor level cleanout assembly with a square adjustable nickel bronze top with 1/8 inch tile recess and an inside caulk outlet.

**** OR ****

Include the following for a square top cleanout with a speedi-set outlet in a linoleum or asphalt tile floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4171 series.
		2.	Description: Cast iron floor level cleanout assembly with a square adjustable nickel bronze top with 1/8 inch tile recess, and a speedi-set outlet.

**** OR ****

Include the following for a round top cleanout with a no-hub outlet in a terrazzo or other poured floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4180 series.
		2.	Description: Cast iron floor level cleanout assembly with round adjustable nickel bronze top with 1/2 inch terrazzo recess and center lifting device, and no-hub outlet.

**** OR ****

Include the following for a round top cleanout with an inside caulk outlet in a terrazzo or other poured floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4185 series.
		2.	Description: Cast iron floor level cleanout assembly with round adjustable nickel bronze top with 1/2 inch terrazzo recess and an inside caulk outlet.

**** OR ****

Include the following for a round top cleanout with a speedi-set outlet in a terrazzo or other poured floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4191 series.
		2.	Description: Cast iron floor level cleanout assembly with round adjustable nickel bronze top with 1/2 inch terrazzo recess and a speedi-set outlet.

**** OR ****

Include the following for a square top cleanout with a no-hub outlet in a terrazzo or other poured floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4200 series.
		2.	Description: Cast iron floor level cleanout assembly with square adjustable nickel bronze top with 1/2 inch terrazzo recess and no-hub outlet.

**** OR ****

Include the following for a square top cleanout with an inside caulk outlet in a terrazzo or other poured floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4205 series.
		2.	Description: Cast iron floor level cleanout assembly with square adjustable nickel bronze top with 1/2 inch terrazzo recess and an inside caulk outlet.

**** OR ****

Include the following for a square top cleanout with a speedi-set outlet in a terrazzo or other poured floor with foot and medium load wheeled traffic.

	A.	Cleanout:
		1.	Model: No. 4211 series.
		2.	Description: Cast iron floor level cleanout assembly with square adjustable nickel bronze top with 1/2 inch terrazzo recess and a speedi-set outlet.

**** OR ****

Include the following for a round top cleanout with a no-hub outlet in an unfinished floor with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4220 series.
		2.	Description: Cast iron floor level cleanout assembly with extra heavy duty, round, adjustable, scoriated, secured cast iron top and no-hub outlet.

**** OR ****

Include the following for a round top cleanout with an inside caulk outlet in an unfinished floor with heavy load traffic.
	A.	Cleanout:
		1.	Model: No. 4225 series.
		2.	Description: Cast iron floor level cleanout assembly with extra heavy duty, round, adjustable, scoriated, secured cast iron top and an inside caulk outlet.

**** OR ****

Include the following for a round top cleanout with a speedi-set outlet in an unfinished floor with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4231 series.
		2.	Description: Cast iron floor level cleanout assembly with extra heavy duty, round, adjustable, scoriated, secured cast iron top and a speedi-set outlet.

**** OR ****

Include the following for a tractor cover cleanout with a no-hub outlet in an outside area or unfinished floor with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4240 series.
		2.	Description: Cast iron floor level cleanout assembly with heavy duty, round, adjustable, scoriated cast iron top with non-tilt tractor cover and no-hub outlet.

**** OR ****

Include the following for a tractor cover cleanout with an inside caulk outlet in an unfinished floor with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4245 series.
		2.	Description: Cast iron floor level cleanout assembly with heavy duty, round, adjustable, scoriated cast iron top, non-tilt tractor cover, and an inside caulk outlet.

**** OR ****

Include the following for a tractor cover cleanout with a speedi-set outlet in an unfinished floor with heavy load traffic.

	A.	Cleanout:
		1.	Model: No. 4237 series or No. 4239 series.
		2.	Description: Cast iron floor level cleanout assembly with heavy duty, round, adjustable, scoriated cast iron top, non-tilt tractor cover, and a speedi-set outlet.

**** OR ****

Include the following for a round flanged cleanout with a no-hub outlet in a yard area or unfinished interior area.

	A.	Cleanout:
		1.	Model: No. 4250 series.
		2.	Description: Cast iron cleanout and double flanged housing with heavy duty, secured, scoriated cast iron cover with lifting device.

**** OR ****

Include the following for a round flanged cleanout with an inside caulk outlet in a yard area or unfinished interior area.

	A.	Cleanout:
		1.	Model: No. 4255 series.
		2.	Description: Cast iron cleanout and double flanged housing with heavy duty, secured, scoriated cast iron cover with lifting device and an inside caulk outlet.

**** OR ****

Include the following for a round flanged cleanout with a speedi-set outlet in a yard area or unfinished interior area.

	A.	Cleanout:
		1.	Model: No. 4261 series.
		2.	Description: Cast iron cleanout and double flanged housing with heavy duty, secured, scoriated cast iron cover with lifting device, and a speedi-set outlet.

**** OR ****

Include the following for an extension type cleanout for non-traffic areas with a no-hub outlet.

	A.	Cleanout:
		1.	Model: No. 4280 series.
		2.	Description: Cast iron extension type cleanout with closure plug.

**** OR ****

Include the following for an extension type cleanout for non-traffic areas with an inside caulk outlet.

	A.	Cleanout:
		1.	Model: No. 4285 series.
		2.	Description: Cast iron extension type cleanout with closure plug and an inside caulk outlet.

**** OR ****

Include the following for an extension type cleanout with a speedi-set outlet.

	A.	Cleanout:
		1.	Model: No. 4291 series.
		2.	Description: Cast iron extension type cleanout with closure plug and a speedi-set outlet.

**** OR ****

Include the following for a cleanout with a medium duty, large access cover where cast iron finish is acceptable and adjustment for floor level is desired.

	A.	Cleanout:
		1.	Model: No. 4313 series.
		2.	Description: Cast iron flanged body and round adjustable top with scoriated, loose set, medium duty, cast iron cover, taper thread bronze closure plug, flashing collar, and an inside caulk or threaded outlet.  

**** OR ****

Include the following for a cleanout with a heavy duty, large access cover where cast iron finish is acceptable and adjustment for floor level is desired.

	A.	Cleanout:
		1.	Model: No. 4318 series.
		2.	Description: Cast iron flanged body and round adjustable top with scoriated, loose set, heavy duty, non-tilt, cast iron cover, taper thread bronze closure plug, flashing collar, and an inside caulk or threaded outlet.  

**** OR ****

Include the following for a cleanout with a medium duty, large access cover where cast iron finish is acceptable and adjustment for floor level is not required.

	A.	Cleanout:
		1.	Model: No. 4333 series.
		2.	Description: Cast iron flanged body and round non-adjustable top with scoriated, loose set, medium duty, cast iron cover, taper thread bronze closure plug, flashing collar, and an inside caulk or threaded outlet.  

**** OR ****

Include the following for a cleanout with a heavy duty, large access cover where cast iron finish is acceptable and adjustment for floor level not required.

	A.	Cleanout:
		1.	Model: No. 4338 series.
		2.	Description: Cast iron flanged body and round non-adjustable top with scoriated, loose set, heavy duty, non-tilt, cast iron cover, taper thread bronze closure plug, flashing collar, and an inside caulk or threaded outlet.  

**** OR ****

Include the following for a wide flange cleanout where a waterproof covering is to be applied and a wide area is required for bonding/support.

	A.	Cleanout:
		1.	Model: No. DX4343 series.
		2.	Description: Cast iron wide flange body with solid, secured, scoriated cover and taper thread bronze closure plug.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping where quick and easy removal is desired.

	A.	Cleanout:
		1.	Model: No. 4400.
		2.	Description: Cast iron caulk ferrule and cast iron lead seal plug.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping where quick and easy removal is desired in a finished wall.

	A.	Cleanout:
		1.	Model: No. 4402.
		2.	Description: Cast iron caulk ferrule, cast iron lead seal plug, and stainless steel round cover and screw.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping.

	A.	Cleanout:
		1.	Model: No. 4420.
		2.	Description: Cast iron spigot ferrule with cast bronze taper thread plug.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping in a finished wall.

	A.	Cleanout:
		1.	Model: No. 4422.
		2.	Description: Cast iron spigot ferrule with cast bronze taper thread plug and stainless steel round cover and screw.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping where quick and easy removal is required in tile, masonry or drywall, with square face-of-wall cover.

	A.	Cleanout:
		1.	Model: No. 4430.
		2.	Description: Cast iron ferrule with cast iron lead seal plug, with chrome plated bronze square frame and secured face-of-wall cover.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping where quick and easy removal is required in plaster or wet wall construction, with square flush-with-wall cover.

	A.	Cleanout:
		1.	Model: No. 4431.
		2.	Description: Cast iron ferrule with cast iron lead seal plug, with chrome plated bronze square frame and secured flush-with-wall cover.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping where quick and easy removal is required in tile, masonry or drywall, with round face-of-wall cover.

	A.	Cleanout:
		1.	Model: No. 4432.
		2.	Description: Cast iron ferrule with cast iron lead seal plug, with chrome plated bronze round frame and secured face-of-wall cover.

**** OR ****

Include the following for an above ground caulk ferrule cleanout in hub openings in drainage piping where quick and easy removal is required in plaster or wet wall construction, with round flush-with-wall cover.

	A.	Cleanout:
		1.	Model: No. 4433.
		2.	Description: Cast iron ferrule with cast iron lead seal plug, with chrome plated bronze round frame and secured flush-with-wall cover.

**** OR ****

Include the following for an above ground spigot ferrule cleanout in hub openings in drainage piping in tile, masonry or drywall, with square face-of-wall cover.

	A.	Cleanout:
		1.	Model: No. 4434.
		2.	Description: Cast iron spigot ferrule with cast bronze taper threaded plug, with chrome plated bronze square frame and secured face-of-wall cover.

**** OR ****

Include the following for an above ground spigot ferrule cleanout in hub openings in drainage piping in plaster or wet wall construction, with square flush-with-wall cover.

	A.	Cleanout:
		1.	Model: No. 4435.
		2.	Description: Cast iron spigot ferrule with cast bronze taper threaded plug, with chrome plated bronze square frame and secured flush-with-wall cover.

**** OR ****

Include the following for an above ground spigot ferrule cleanout in hub openings in drainage piping in tile, masonry or drywall, with round face-of-wall cover.

	A.	Cleanout:
		1.	Model: No. 4436.
		2.	Description: Cast iron spigot ferrule with cast bronze taper threaded plug, with chrome plated bronze round frame and secured face-of-wall cover.

**** OR ****

Include the following for an above ground spigot ferrule cleanout in hub openings in drainage piping in plaster or wet wall construction, with round flush-with-wall cover.

	A.	Cleanout:
		1.	Model: No. 4437.
		2.	Description: Cast iron spigot ferrule with cast bronze taper threaded plug, with chrome plated bronze round frame and secured flush-with-wall cover.

**** OR ****

Include the following for a caulk ferrule cleanout for a hub opening in drainage piping where a round floor or wall cover is required. 

	A.	Cleanout:
		1.	Model: No. 4438.
		2.	Description: Cast iron caulk ferrule with cast iron lead seal plug and secured, round, scoriated nickel bronze cover and frame with anchor lugs.

**** OR ****

Include the following for a caulk ferrule cleanout for a hub opening in drainage piping where a square floor or wall cover is required. 

	A.	Cleanout:
		1.	Model: No. 4439.
		2.	Description: Cast iron caulk ferrule with cast iron lead seal plug and secured, square, scoriated nickel bronze cover and frame with anchor lugs.

**** OR ****

Include the following for a caulk ferrule cleanout with a taper thread plug for a hub opening in drainage piping where a round floor or wall cover is required. 

	A.	Cleanout:
		1.	Model: No. 4440.
		2.	Description: Cast iron caulk ferrule with cast bronze taper thread plug and secured, round, scoriated nickel bronze cover and frame with anchor lugs.

**** OR ****

Include the following for a caulk ferrule cleanout with a taper thread plug for a hub opening in drainage piping where a square floor or wall cover is required. 

	A.	Cleanout:
		1.	Model: No. 4441.
		2.	Description: Cast iron caulk ferrule with cast bronze taper thread plug and secured, square, scoriated nickel bronze cover and frame with anchor lugs.

**** OR ****

Include the following for a full calibre caulk ferrule cleanout for a hub opening in drainage piping. 

	A.	Cleanout:
		1.	Model: No. 4450.
		2.	Description: Cast iron full calibre caulk ferrule with cast bronze taper thread plug.

**** OR ****

Include the following for a full calibre caulk ferrule cleanout for a hub opening in drainage piping in a finished wall. 

	A.	Cleanout:
		1.	Model: No. 4452.
		2.	Description: Cast iron full calibre caulk ferrule with cast bronze taper thread plug and stainless steel round cover and screw.

**** OR ****

Include the following for an above ground cleanout plug in female pipe size openings in drainage piping.

	A.	Cleanout Plug:
		1.	Model: No. 4470.
		2.	Description: Cast bronze taper thread plug.

**** OR ****

Include the following for an above ground cleanout plug in female pipe size openings in drainage piping in a finished wall.

	A.	Cleanout:
		1.	Model: No. 4472.
		2.	Description: Cast bronze taper thread plug with stainless steel round cover and screw.

**** OR ****

Include the following for a cleanout in concealed drainage lines that allows for testing of piping above through the use of an internal threading inside the tee.

	A.	Cleanout Plug:
		1.	Model: No. 4505.
		2.	Description: Cast iron cleanout tee with internal threading, 1/2 NPT test port with raised head plug, and countersunk taper threaded bronze plug.

**** OR ****

Include the following for a cleanout in concealed drainage lines.

	A.	Cleanout Plug:
		1.	Model: No. 4510 series.
		2.	Description: Cast iron cleanout tee and cast iron countersunk plug.

**** OR ****
Include the following for a cleanout in concealed drainage lines in a finished wall.

	A.	Cleanout Plug:
		1.	Model: No. 4530 series.
		2.	Description: Cast iron cleanout tee and cast iron countersunk plug with stainless steel round cover and screw.

**** OR ****

Include the following for a cleanout in concealed drainage lines in tile, masonry or drywall construction with square face-of-wall cover.

	A.	Cleanout Plug:
		1.	Model: No. 4550 series.
		2.	Description: Cast iron cleanout tee and cast iron countersunk plug with chrome plated bronze square frame and secured face-of-wall cover.

**** OR ****

Include the following for a cleanout in concealed drainage lines in plaster or wet wall construction with square face-of-wall cover.

	A.	Cleanout Plug:
		1.	Model: No. 4555 series.
		2.	Description: Cast iron cleanout tee and cast iron countersunk plug with chrome plated bronze square frame and secured flush-with-wall cover.

Insert the following under “Accessories.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting http://www.baldwinhardware.comspecific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a shallow access cover to conceal cleanout closure in finished walls.    

	A.	Access Cover:
		1.	Model: No. 4710.
		2.	Description: Stainless steel shallow cover with center screw.

**** OR ****

Include the following for a deep access cover to conceal cleanout closure in finished walls where the cleanout plug protrudes beyond the finished wall surface.    

	A.	Access Cover:
		1.	Model: No. 4715.
		2.	Description: Chrome plated bronze deep cover with center screw.

**** OR ****

Include the following for a round access cover to conceal cleanout plugs, valves, controls or equipment in tile, masonry or drywall construction.    

	A.	Access Cover:
		1.	Model: No. 4720.
		2.	Description: Chrome plated bronze round frame and secured face-of-wall cover with anchoring lugs.

**** OR ****

Include the following for a round access cover to conceal cleanout plugs, valves, controls or equipment in plaster or wet wall construction.    

	A.	Access Cover:
		1.	Model: No. 4725.
		2.	Description: Chrome plated bronze round frame and secured flush-with-wall cover with anchoring lugs.

**** OR ****

Include the following for a square access cover to conceal cleanout plugs, valves, controls or equipment in tile, masonry, or drywall construction.    

	A.	Access Cover:
		1.	Model: No. 4730.
		2.	Description: Chrome plated bronze square frame and secured face-of-wall cover with anchoring lugs.

**** OR ****

Include the following for a square access cover to conceal cleanout plugs, valves, controls or equipment in plaster or wet wall construction.    

	A.	Access Cover:
		1.	Model: No. 4735.
		2.	Description: Chrome plated bronze square frame and secured flush-with-wall cover with anchoring lugs.

**** OR ****

Include the following for a square access cover and box to conceal flush valves in tile, masonry or drywall construction, provide a means of actuating the valves by handle, push button or pedal, and provide access from the toilet room to adjust or maintain the valve.    

	A.	Access Cover:
		1.	Model: No. 4740.
		2.	Description: Chrome plated bronze square frame and secured face-of-wall cover with aluminum frame and adjustable anchoring lugs.

**** OR ****

Include the following for a square access cover and box to conceal flush valves in plaster or wet wall construction, provide a means of actuating the valves by handle, push button or pedal, and provide access from the toilet room to adjust or maintain the valve. 

	A.	Access Cover:
		1.	Model: No. 4745.
		2.	Description: Chrome plated bronze square frame and secured flush-with-wall cover with aluminum frame and adjustable anchoring lugs.

**** OR ****

Include the following for a square access cover to conceal cleanout plugs, valves, controls or equipment in tile, masonry, or drywall walls or ceilings.    

	A.	Access Cover:
		1.	Model: No. 4760.
		2.	Description: Prime coated steel concealed hinge, face-of-wall, access cover with screwdriver operated latch.

**** OR ****
Include the following for a square access cover to conceal cleanout plugs, valves, controls or equipment in tile or unpainted surfaces.  

	A.	Access Cover:
		1.	Model: No. 4762.
		2.	Description: No. 4 satin finish 18-8 stainless steel concealed hinge, face-of-wall, access cover with screwdriver operated latch.

**** OR ****

Include the following for a square access cover to conceal cleanout plugs, valves, controls or equipment in wet walls; or plaster or terrazzo walls or ceilings.  

	A.	Access Cover:
		1.	Model: No. 4765.
		2.	Description: Prime coated steel concealed hinge, flush-with-wall, access cover with screwdriver operated latch.

**** OR ****

Include the following for a square access cover to conceal cleanout plugs, valves, controls or equipment in terrazzo or unpainted surfaces.  

	A.	Access Cover:
		1.	Model: No. 4767.
		2.	Description: No. 4 satin finish 18-8 stainless steel concealed hinge, flush-with-wall, access cover with screwdriver operated latch.

**** OR ****

Include the following for an access cover in concrete floors and/or surfaced areas subject to ordinary foot traffic and normal loadings.  

	A.	Access Cover:
		1.	Model: No. 4810.
		2.	Description: Secured scoriated nickel bronze cover and frame with anchor lugs.

**** OR ****

Include the following for an access cover in exterior grade areas; parking lots and driveways.  

	A.	Access Cover:
		1.	Model: No. 4880.
		2.	Description: Cast iron surface level access cover assembly with lifting device.

**** OR ****

Include the following for a floor cleanout in drainage lines where the cover is required to be watertight.  

	A.	Access Cover:
		1.	Model: No. 4890.
		2.	Description: Nickel bronze round deck plug with polished, scoriated, spanner wrench cover.

**** OR ****

Include the following for a floor cleanout in drainage lines where the cover is required to be watertight with a large bearing surface for traffic deck coatings.  

	A.	Access Cover:
		1.	Model: No. DX4890.
		2.	Description: Nickel bronze round deck plug with large flange and polished, scoriated, spanner wrench cover.

**** OR ****

Include the following for an access cover in concrete, terrazzo or tile floors.  

	A.	Access Cover:
		1.	Model: No. 4910. 
		2.	Description: Cast aluminum scoriated secured top access cover with lifting device and perforated concrete flange.  

**** OR ****

Include the following for an access cover in concrete, terrazzo or tile floors for areas of frequently used valves and equipment.  

	A.	Access Cover:
		1.	Model: No. 4915. 
		2.	Description: Cast aluminum scoriated hinged secured top access cover and perforated concrete flange.  

**** OR ****

Include the following for an access cover to provide access to cleanouts, valves, controls or equipment in concrete floors and surfaced areas subject to normal foot traffic.

	A.	Access Cover:
		1.	Model: No. 4930. 
		2.	Description: Square nickel bronze frame and secured scoriated cover.  

**** OR ****

Include the following for an access cover to provide access to frequently used cleanouts, valves, controls or equipment in concrete floors and surfaced areas subject to normal foot traffic.

	A.	Access Cover:
		1.	Model: No. 4940. 
		2.	Description: Square nickel bronze frame and hinged scoriated cover with locking device.  
 
PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.