CSMV-3
Valve MV17-3 90 gpm (341 lpm)

CSMV-3-TBV
Valve MV17-3 90 gpm (341 lpm) with TBV (Thermostatic Balancing Valve)

CSMV-3-D-1-6-0-0-0.rfa
Valve MV17-3 90 gpm (341 lpm); 3/4" Return Pipe Size; Pump with AquaStat Control; Thermostatic Limiting Balancing Valve

CSMV-5-G-1-0-0
Valve MV17-5 225 gpm (852 lpm); 1-1/2" Return Pipe Size; Pump with AquaStat Control; No Auto Balancing Valve; No Cold Water By-Pass

CSMV_Series_Command_Station_DWGzipped.txt
This text file describing contents