CLOSET SUPPORTS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying closet supports. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a siphon jet water closet where water closet must be elevated 3 inches higher than normal rough-in height.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0100 Series.
		2.	Description: Adjustable hi-set elevated support for 3 inch higher than normal rough-in height.

**** OR ****

Include the following for a siphon jet water closet where water closet must be elevated 3 inches higher than normal rough-in height, in a back-to-back configuration.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0100D Series.
		2.	Description: Double adjustable hi-set elevated support for 3 inch higher than normal rough-in height.

**** OR ****

Include the following for a siphon jet water closet where water closet must be elevated 3 inches higher than normal rough-in height, with a no-hub connection.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0100Y Series.
		2.	Description: Adjustable hi-set elevated, no-hub, support for 3 inch higher than normal rough-in height.

**** OR ****

Include the following for a siphon jet water closet where water closet must be elevated 3 inches higher than normal rough-in height, with a no-hub connection in a back-to-back configuration.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0100DY Series.
		2.	Description: Double adjustable hi-set elevated, no-hub, support for 3 inch higher than normal rough-in height.

**** OR ****

Include the following for single-pour floor construction for a siphon jet water closet.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0200 Series.
		2.	Description: Adjustable rough-in support for single-pour floor construction.

**** OR ****

Include the following for single-pour floor construction for a siphon jet water closet in a back-to-back configuration.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0200D Series.
		2.	Description: Double adjustable rough-in support for single-pour floor construction.

**** OR ****

Include the following for single-pour floor construction for a siphon jet water closet without a no-hub connection.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0200Y Series.
		2.	Description: Adjustable rough-in, no-hub, support for single-pour floor construction.

**** OR ****

Include the following for single-pour floor construction for a siphon jet water closet without a no-hub connection in a back-to-back configuration.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: 0200DY Series.
		2.	Description: Double adjustable rough-in, no-hub, support for single-pour floor construction.

**** OR ****

Include the following for the adjustable series for a blowout type water closet.

	A.	Wall-Hung Blowout Water Closet Support:
		1.	Model: 0300 Series.
		2.	Description: Adjustable rough-in support for single pour floor construction.

**** OR ****

Include the following for the adjustable series for a blowout type water closet in a back-to-back configuration.

	A.	Wall-Hung Blowout Water Closet Support:
		1.	Model: 0300D Series.
		2.	Description: Double adjustable rough-in support for single pour floor construction.
**** OR ****

Include the following for the adjustable series for a blowout type water closet with a no-hub connection.

	A.	Wall-Hung Blowout Water Closet Support:
		1.	Model: 0300Y Series.
		2.	Description: Adjustable rough-in, no-hub, support for single pour floor construction.

**** OR ****

Include the following for the adjustable series for a blowout type water closet with a no-hub connection in a back-to-back configuration.

	A.	Wall-Hung Blowout Water Closet Support:
		1.	Model: 0300DY Series.
		2.	Description: Double adjustable rough-in, no-hub, support for single pour floor construction.

**** OR ****

Include the following for the adjustable series for a floor-mounted back outlet type water closet.  

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 200 or 300 series.
		2.	Description: Adjustable rough-in support for connection to a floor mounted back outlet type water closet. 

**** OR ****

Include the following for the adjustable series for a floor-mounted back outlet type water closet in a back-to-back configuration.  

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 200D or 300D series.
		2.	Description: Double adjustable rough-in support for connection to a floor mounted back outlet type water closet. 

**** OR ****

Include the following for the adjustable series for a floor-mounted back outlet type water closet with a no-hub connection.  

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 200Y or 300Y series.
		2.	Description: Adjustable rough-in, no-hub, support for connection to a floor mounted back outlet type water closet. 

**** OR ****

Include the following for the adjustable series for a floor-mounted back outlet type water closet in a back-to-back configuration with a no-hub connection.  

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 200DY or 300DY series.
		2.	Description: Double adjustable rough-in, no-hub, support for connection to a floor mounted back outlet type water closet. 

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a commercial setting.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 0400.
		2.	Description: Compact rough-in support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a commercial setting in a back-to-back configuration.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 0400D.
		2.	Description: Double compact rough-in support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a commercial setting, with a no-hub connection.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 0400Y.
		2.	Description: Compact rough-in, no-hub, support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a commercial setting, with a no-hub connection in a back-to-back configuration.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 0400DY.
		2.	Description: Double compact rough-in, no-hub, support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a residential or light commercial setting.

	A.	Wall-Hung Residential or Light Commercial Siphon Jet Water Closet Support:
		1.	Model: 530 or 540 series.
		2.	Description: Compact rough-in support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a residential or light commercial setting, with a no-hub connection.

	A.	Wall-Hung Residential or Light Commercial Siphon Jet Water Closet Support:
		1.	Model: 540D series.
		2.	Description: Double compact rough-in support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a residential or light commercial setting, with a no-hub connection.

	A.	Wall-Hung Residential or Light Commercial Siphon Jet Water Closet Support:
		1.	Model: 530Y or 540Y series.
		2.	Description: Compact rough-in, no-hub, support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a siphon jet water closet in a residential or light commercial setting, with a no-hub connection.

	A.	Wall-Hung Residential or Light Commercial Siphon Jet Water Closet Support:
		1.	Model: 540DY series.
		2.	Description: Double compact rough-in, no-hub, support with vertical offset or center line fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a stud-mounted siphon jet water closet and no fitting is required.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 548. 
		2.	Description: Compact rough-in support without fitting with stud mount frame. 

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for stud-mounted siphon jet water closets in a back-to-back configuration and no fitting is required.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 548D. 
		2.	Description: Double compact rough-in support without fitting with stud mount frame. 

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for a floor-mounted siphon jet water closet and no fitting is required.

	A.	Floor-Mounted Siphon Jet Water Closet Support:
		1.	Model: No. 548F. 
		2.	Description: Compact rough-in support without fitting with floor mount frame. 

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for floor-mounted siphon jet water closets in a back-to-back configuration and no fitting is required.

	A.	Floor-Mounted Siphon Jet Water Closet Support:
		1.	Model: No. 548FD. 
		2.	Description: Double compact rough-in support without fitting with floor mount frame. 

**** OR ****

Include the following for a stud-mounted residential type water closet.  

	A.	Wall-Hung Residential Water Closet Support:
		1.	Model: 0550 series.
		2.	Description: Siphon jet support with waste fitting and adjustable steel
			face plate. 

**** OR ****

Include the following for stud-mounted residential type water closets in a back-to-back configuration.  

	A.	Wall-Hung Residential Water Closet Support:
		1.	Model: 0550D series.
		2.	Description: Double siphon jet support with waste fitting and adjustable steel
			face plate. 

**** OR ****

Include the following for a floor-mounted residential or light commercial type water closet.  

	A.	Floor-Mounted Residential or Light Commercial Water Closet Support:
		1.	Model: 0550F series.
		2.	Description: Siphon jet support with waste offset fitting and extra heavy cast iron
			face plate. 

**** OR ****

Include the following for floor-mounted residential or light commercial type water closets in a back-to-back configuration.  

	A.	Floor-Mounted Residential or Light Commercial Water Closet Support:
		1.	Model: 0550FD series.
		2.	Description: Double siphon jet support with waste offset fitting and extra heavy cast iron
			face plate. 

**** OR ****

Include the following for a face plate type fixture support for a siphon jet water closet.

	A.	Wall-Hung Siphon Jet Water Closet Support:
		1.	Model: No. 0600.
		2.	Description: Face plate support without fitting.

**** OR ****

Include the following for a face plate type fixture support for a blowout type water closet.

	A.	Wall-Hung Blowout Water Closet Support:
		1.	Model: No. 0620.
		2.	Description: Face plate support without fitting.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for the floor-mounted back outlet type water closet.

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 400 series or No. 670-680.
		2.	Description: Compact rough-in support for connection to a floor-mounted back outlet type water closet.
**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for the floor-mounted back outlet type water closet in a back-to-back configuration.

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 400D series or No. 670D-680D.
		2.	Description: Double compact rough-in support for connection to a floor-mounted back outlet type water closet.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for the floor-mounted back outlet type water closet with a no-hub connection.

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 400Y series or No. 670Y-680Y.
		2.	Description: Compact rough-in, no-hub, support for connection to a floor-mounted back outlet type water closet.

**** OR ****

Include the following where the furred space is not sufficient for the adjustable series for the floor-mounted back outlet type water closet in a back-to-back configuration with a no-hub connection.

	A.	Floor-Mounted Back Outlet Water Closet Support:
		1.	Model: 400DY series or No. 670DY-680DY.
		2.	Description: Double compact rough-in, no-hub, support for connection to a floor-mounted back outlet type water closet.

PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.