**Accessory: Modular Privacy Compartments for Commercial Showers  
Specify with -MS Option when ordering shower**

File name: DPMOD.DWG

A picture containing text, crossword puzzle

Description automatically generated

|  |  |  |
| --- | --- | --- |
| 3 Station Corner Layout:  Acorn 110 Shower,  each with individual dressing compartment | 6 Station (Against-Single-Wall) Layout: Acorn 130 Shower,  each with individual dressing compartment |  |
| 4-Station (Between-Two-Walls) Layout: Column Shower can be Acorn 640, 740, 940 | 4-Station (Against-Single-Wall) Layout: Column Shower can be Acorn 640, 740, 940 | 4-Station (Middle of Room) Layout: Column Shower can be Acorn 640, 740, 940 |
| 4-Station (Against-Single-Wall) Layout: Column Shower can be Acorn 640, 740, 940; each with individual dressing compartment. | 4-Station (Against-Single-Wall) Layout – Alternate 1: Column Shower can be Acorn 640, 740, 940; each with individual dressing compartment. |  |
| 4-Station (Against-Single-Wall) Layout – Alternate 2: Column Shower can be Acorn 640, 740, 940; each with individual dressing compartment. | 4-Station (Middle of Room) Layout:  Column Shower can be Acorn 640, 740, 940; each with individual dressing compartment. |  |

File name: DPMOD1.DWG

Diagram, engineering drawing

Description automatically generated

|  |  |
| --- | --- |
| 4-Station (Middle of Room) Layout: Column Shower can be Acorn 640, 740, 940; each with two dressing compartment. | 8-Station (Between-2-Walls) Layout: Two 4-Station Column Showers can be Acorn 640, 740, 940; each with individual dressing compartment |
| 8-Station (Against-Single-Wall) Layout: Two 4-Station Column Showers can be Acorn 640, 740, 940; each with individual dressing compartment | 8-Station (Middle of Room) Layout: Two 4-Station Column Showers can be Acorn 640, 740, 940; each with individual dressing compartment |
| 12-Station (Between-2-Walls) Layout: Three 4-Station Column Showers can be Acorn 640, 740, 940 each with individual dressing compartment |  |

File name: DPMOD3.DWG

Diagram, engineering drawing

Description automatically generated

|  |  |
| --- | --- |
| 10-Station (Between-Two-Wall) Layout:  Two Individual Wall Shower could be Acorn 410, 420, 450, 530; Two 4-Station Column Showers could be Acorn 640, 740, 940; each with individual dressing compartments | 10-Station (Against-Single-Wall) Layout:  Two Individual Wall Shower could be Acorn 410, 420, 450, 530; Two 4-Station Column Showers could be Acorn 640, 740, 940; each with individual dressing compartments |
| 6-Station (Against-Single-Wall) Layout:  Six Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments | 4-Station (Against-Single-Wall) Layout  Four Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |
| 6-Station Corner Layout  Six Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |  |
|  | 6-Station Alcove Layout  Six Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |

File name: DPMOD4.DWG

Diagram, engineering drawing

Description automatically generated

|  |  |  |
| --- | --- | --- |
| 4-Station Corner Layout:  Four Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments | 4-Station Alcove Layout:  Four Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |  |
| 4-Station (Against-Single-Wall) Layout: Four Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |  |  |
| 4-Station Alcove Layout:  Four Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |  |  |
| 3-Station Alcove Layout:  Three Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments | 2-Station (Against-Single-Wall) Layout: Two Individual Wall Showers could Acorn 410, 420, 450, 530; each with two dressing compartments |  |
| 2-Station (Against-Single-Wall) Layout: Two Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments | 2-Station Alcove Layout: Two Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments | 2-Station Corner Layout: Two Individual Wall Showers could Acorn 410, 420, 450, 530; each with individual dressing compartments |